#

Free vector and raster map data at 1:10m, 1:50m, and 1:110m scales
Search for:

- Home
- Features
- Downloads
- Blog
- Forums
- Corrections
- About

« 1:10m Physical Vectors « Downloads

## Bathymetry

Nested polygons for each depth created from SRTM Plus.
Download all (14.86 MB) version 4.1.0
Download 0m (2.86 MB) version 4.0.0
Download 200 m (1.14 MB) version 4.0.0
Download 1,000 m (741.08 KB) version 4.0.0
Download 2,000 m (1.23 MB) version 4.0.0
Download 3,000 m (2.41 MB) version 4.0.0
Download 4,000 m (3.43 MB) version 4.0.0
Download 5,000 m (2.72 MB) version 4.0.0
Download 6,000 m (279.02 KB) version 4.0.0
Download 7,000 m (35.5 KB) version 4.0.0
Download 8,000 m (17.78 KB) version 4.0.0
Download 9,000 m (12.85 KB) version 4.0.0
Download 10,000 m (8.95 KB) version 4.0.0

About

Nested polygons at 0, -200, -1,000, -2,000, -3,000, -4,000, -5,000, -6,000, -7,000, -8,000, -9,000, and -10,000 meters. Created from SRTM Plus. The minus 2oo meter bathymetry layer is buffered slightly around all coastlines to avoid coastline overlaps. Isobaths surrounding islands, seamounts, and near other steep slopes received considerable manual generalization to improve legibility.

(below) North Atlantic ocean depth bathymetry off Spain (composite of all bathymetry files).

Issues

None.

Resources

SRTM Plus elevation data

Version History

- 4.1.0
- 4.0.0
- 2.0.0
- 1.3.0
- 1.1.0
- 1.0.0

The master changelog is available on Github »